function joy_z(argument0) {
	// joy_z(id)
	//Returns the position (from -1 to 1) of the third axis on the joystick.

	return external_call(global.ljoyAxis, argument0, 2);

	//  NOTE THAT JOY'S IDs START FROM ZERO AND NOT ONE!!!




}
